Samuel Bailey

Assignment 2-2 Questions

What does pwmled2 set the PWM period to?

This sets the PWD to open.

Which PWM\_xxx() function sets the PWM period?

PWM\_open

Which PWM\_xxx() function sets the PWM duty cycle?

PWM\_setDuty()

What is the purpose of the while(1) loop in pwmled2?

Iteration of program to keep it running.

What is the purpose of usleep() in the while(1) loop?

Suspends threads for microseconds to not overload